IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2017-10-15T19:21:28"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20161004_0715(x64) - Exporter 16.3.0.0 - Interface alternative d'export 16.3.0.0"
Application: "Autodesk Revit 2016 (FRA)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (FRA)"

People and organizations
  Person "ced.dziuba@gmail.com" of Organization (no name given)
  Owner history of Person "ced.dziuba@gmail.com" of Organization (no name given) | application "Autodesk Revit 2016 (FRA)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (FRA)" | change NOCHANGE | created 1508082362 (2017-10-15T15:46:02Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT | long name "CONSTRUCTION D'UNE ECOLE A AUBAREDE (65)"
  IFCSITE "Default" | latitude 48° 52′ 53.759999″ | longitude 2° 25′ 58.079999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Entrer l'adresse ici", "Paris", "France"
      IFCBUILDINGSTOREY "1 - RDC" | long name "1 - RDC" | elevation 1.94210219716249E-13
        contains 4 elements
          1 x IFCROOF | object type "Toit de base:Toit - 200 mm" | names: "Toit de base:Toit - 200 mm:194313" | parts: 4 IFCSLAB | property sets: Pset_RoofCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Ferme Charpente Tradi_Aubarède" | object type "Ferme Charpente Tradi_Aubarède" | names: "Ferme Charpente Tradi_Aubarède:Ferme Charpente Tradi_Aubarède:276327" | material: "bois de charpente" | property sets: Pset_BuildingElementProxyCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Ferme Charpente Tradi_Aubarède" | object type "Ferme Charpente Tradi_Aubarède" | names: "Ferme Charpente Tradi_Aubarède:Ferme Charpente Tradi_Aubarède:277460", "Ferme Charpente Tradi_Aubarède:Ferme Charpente Tradi_Aubarède:277599" | material: "bois de charpente" | property sets: Pset_BuildingElementProxyCommon
      IFCBUILDINGSTOREY "2 - Arase murs" | long name "2 - Arase murs" | elevation 3.51500000000008
        contains 2 elements
          1 x IFCBEAM | object type "Poutre - Bois d'oeuvre+support:Panne 80x220:281430" | names: "Poutre - Bois d'oeuvre+support:Panne 80x220:281406" | material: "bois de charpente" | property sets: Pset_BeamCommon
          1 x IFCBEAM | object type "Poutre - Bois d'oeuvre+support:Entrait 80x200:283217" | names: "Poutre - Bois d'oeuvre+support:Entrait 80x200:282583" | material: "bois de charpente" | property sets: Pset_BeamCommon

Types
  IFCBUILDINGELEMENTPROXYTYPE "Ferme Charpente Tradi_Aubarède" | 1 occurrence | material: "bois de charpente"
  IFCBUILDINGELEMENTPROXYTYPE "Ferme Charpente Tradi_Aubarède" | 2 occurrences | material: "bois de charpente"

Property sets
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 346.8696 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Toit - 200 mm" (IFCIDENTIFIER)
    TotalArea = 362.14249426232 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 16.6992442339936 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Toit - 200 mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 16.6992442339937 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Toit - 200 mm" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Reference = "Ferme Charpente Tradi_Aubarède" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Panne 80x220" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 4.225 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Entrait 80x200" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 4.1 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 2 (IFCINTEGER)