IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2017-12-12T18:16:18"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20170927_1515(x64) - Exporter 18.2.0.0 - Interface alternative d'export 18.2.0.0"
Application: "Autodesk Revit 2018 (FRA)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (FRA)"

People and organizations
  Person "ced.dziuba@gmail.com" of Organization (no name given)
  Owner history of Person "ced.dziuba@gmail.com" of Organization (no name given) | application "Autodesk Revit 2018 (FRA)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (FRA)" | change NOCHANGE | created 1513098865 (2017-12-12T17:14:25Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Nom du projet" | phase "Etat du projet"
  IFCSITE "Default" | latitude 48° 51′ 23.807373″ | longitude 2° 21′ 7.999076″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Entrer l'adresse ici", "Paris", "France"
      IFCBUILDINGSTOREY "1 - RDC" | long name "1 - RDC" | elevation 1.94210219716249E-13
        contains 15 elements
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "Raccordement 300 x 300 à face 600 x 600" | object type "Raccordement 300 x 300 à face 600 x 600" | names: "Bouche de reprise:Raccordement 300 x 300 à face 600 x 600:744299", "Bouche de reprise:Raccordement 300 x 300 à face 600 x 600:744490" | property sets: Pset_DistributionFlowElementCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "2200 m3h" | object type "2200 m3h" | names: "Ventilateur d'extraction d'air neuf - Centrifuge - 2200 m3h:2200 m3h:744994" | property sets: Pset_BuildingElementProxyCommon
          5 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Gaine circulaire:Réduction excentrée / Coude segmenté" | object type "Gaine circulaire:Réduction excentrée / Coude segmenté:142430" | names: "Gaine circulaire:Réduction excentrée / Coude segmenté:745143", "Gaine circulaire:Réduction excentrée / Coude segmenté:745212", "Gaine circulaire:Réduction excentrée / Coude segmenté:745222" (+2 more) | property sets: Pset_DistributionFlowElementCommon
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Standard" | object type "Standard" | names: "Gaine RE RU - Joint coulissant:Standard:745145", "Gaine RE RU - Joint coulissant:Standard:745224" | property sets: Pset_DistributionFlowElementCommon
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "5 panneaux 1.5 a" | object type "5 panneaux 1.5 a" | names: "Coude à segments circulaire - Joint coulissant:5 panneaux 1.5 a:745147", "Coude à segments circulaire - Joint coulissant:5 panneaux 1.5 a:745225", "Coude à segments circulaire - Joint coulissant:5 panneaux 1.5 a:745238" | property sets: Pset_DistributionFlowElementCommon
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Standard" | object type "Standard" | names: "Branche circulaire en caoutchouc - Joint coulissant:Standard:745310" | property sets: Pset_DistributionFlowElementCommon
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "Standard" | object type "Standard" | names: "Transformation ronde - Joint coulissant:Standard:745312" | property sets: Pset_DistributionFlowElementCommon

Types
  IFCAIRTERMINALTYPE "Raccordement 300 x 300 à face 600 x 600" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "2200 m3h" | 1 occurrence
  IFCDUCTSEGMENTTYPE "Gaine circulaire:Réduction excentrée / Coude segmenté" | 5 occurrences
  IFCDUCTFITTINGTYPE "Standard" | 2 occurrences
  IFCDUCTFITTINGTYPE "5 panneaux 1.5 a" | 3 occurrences
  IFCDUCTFITTINGTYPE "Standard" | 1 occurrence
  IFCDUCTFITTINGTYPE "Standard" | 1 occurrence

Property sets
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_DistributionFlowElementCommon | properties | on 5 objects (5 IFCFLOWSEGMENT)
    Reference = "Réduction excentrée / Coude segmenté" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 4 objects (4 IFCFLOWFITTING)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 3 objects (3 IFCFLOWFITTING)
    Reference = "5 panneaux 1.5 a" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 2 objects (2 IFCFLOWTERMINAL)
    Reference = "Raccordement 300 x 300 à face 600 x 600" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "2200 m3h" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)