IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView_V2.0, QuantityTakeOffAddOnView]"
Description: "Option [BaseQuantities:On]"
Description: "Option [GridExport:Off]"
Description: "Option [Assemblies:On]"
Description: "Option [Bolts:On]"
Description: "Option [Rebars:On]"
Description: "Option [PourObjects:Off]"
Description: "Option [Welds:Off]"
Description: "Option [SurfaceTreatments:Off]"
Description: "Option [LocationBy:0]"
Description: "Option [ViewColors:On]"
Description: "Option [SectionedSpine:Off]"
Description: "Option [PropertySets:On]"
Description: "Option [Export all:Off]"
File name: "Hangar TP1.ifc"
Time stamp: "2020-04-17T14:07:55"
Author: "DESKTOP-M1HRC43\Christian V"
Organization: "Structural Designer"
Preprocessor: "IFC Database Version: Work"
Originating system: "Tekla Structures Educational 2019i, IFC Export Version: 4.0.0.0 Sep 2 2019"
Application: "Tekla Structures Educational" version "2019i" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation"

People and organizations
  Person "Undefined" id "DESKTOP-M1HRC43\Christian V" of Organization "Trimble Solutions Corporation"
  Owner history of Person "Undefined" id "DESKTOP-M1HRC43\Christian V" of Organization "Trimble Solutions Corporation" | application "Tekla Structures Educational" version "2019i" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1587125268 (2020-04-17T12:07:48Z)
  Owner history of Person "Undefined" id "DESKTOP-M1HRC43\Christian V" of Organization "Trimble Solutions Corporation" | application "Tekla Structures Educational" version "2019i" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1587038400 (2020-04-16T12:00:00Z)
  Owner history of Person "Undefined" id "DESKTOP-M1HRC43\Christian V" of Organization "Trimble Solutions Corporation" | application "Tekla Structures Educational" version "2019i" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1586876400 (2020-04-14T15:00:00Z)
  Owner history of Person "Undefined" id "DESKTOP-M1HRC43\Christian V" of Organization "Trimble Solutions Corporation" | application "Tekla Structures Educational" version "2019i" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1558105200 (2019-05-17T15:00:00Z)
  Owner history of Person "Undefined" id "DESKTOP-M1HRC43\Christian V" of Organization "Trimble Solutions Corporation" | application "Tekla Structures Educational" version "2019i" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1558083600 (2019-05-17T09:00:00Z)
  Owner history of Person "Undefined" id "DESKTOP-M1HRC43\Christian V" of Organization "Trimble Solutions Corporation" | application "Tekla Structures Educational" version "2019i" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1558022400 (2019-05-16T16:00:00Z)
  Owner history of Person "Undefined" id "DESKTOP-M1HRC43\Christian V" of Organization "Trimble Solutions Corporation" | application "Tekla Structures Educational" version "2019i" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1558018800 (2019-05-16T15:00:00Z)
  Owner history of Person "Undefined" id "DESKTOP-M1HRC43\Christian V" of Organization "Trimble Solutions Corporation" | application "Tekla Structures Educational" version "2019i" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1557154800 (2019-05-06T15:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  PLANEANGLEUNIT: RADIAN
  SOLIDANGLEUNIT: STERADIAN
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Undefined"
  IFCSITE "Undefined" | elevation above sea level 0.
    IFCBUILDING "Undefined"
      IFCBUILDINGSTOREY "Undefined" | elevation 0.
        contains 507 elements
          496 x IFCELEMENTASSEMBLY | RIGID_FRAME | names: "Steel Assembly" | parts: 472 IFCBEAM, 210 IFCMECHANICALFASTENER, 111 IFCDISCRETEACCESSORY, 12 IFCPLATE, 10 IFCCOLUMN, 2 IFCMEMBER | property sets: Tekla Assemblages, BaseQuantities
          11 x IFCELEMENTASSEMBLY | REINFORCEMENT_UNIT | names: "SEMELLE", "DALLE" | parts: 41 IFCREINFORCINGBAR, 10 IFCFOOTING, 1 IFCSLAB | property sets: BaseQuantities, Tekla Assemblages

Property sets
  Tekla Assemblages | properties | on 3 objects (3 IFCELEMENTASSEMBLY)
    Finition (no value)
    Niveau Bas Assemblage/Elément béton = "+4.794" (IFCLABEL)
    Niveau Haut Assemblage/Elément béton = "+5.357" (IFCLABEL)
    Poids Assemblage/Elément béton = 66.3 (IFCMASSMEASURE) [KILO GRAM]
    Poids ferraillage Elément béton (no value)
    Position maillage Assemblage/Elément béton = "7-11/A-B" (IFCLABEL)
    Repère Assemblage/Elément béton = "PA27(?)" (IFCLABEL)
  Tekla Assemblages | properties | on 3 objects (3 IFCELEMENTASSEMBLY)
    Finition (no value)
    Niveau Bas Assemblage/Elément béton = "+4.794" (IFCLABEL)
    Niveau Haut Assemblage/Elément béton = "+5.357" (IFCLABEL)
    Poids Assemblage/Elément béton = 66.3 (IFCMASSMEASURE) [KILO GRAM]
    Poids ferraillage Elément béton (no value)
    Position maillage Assemblage/Elément béton = "7-11/B-C" (IFCLABEL)
    Repère Assemblage/Elément béton = "PA27(?)" (IFCLABEL)
  Tekla Assemblages | properties | on 3 objects (3 IFCELEMENTASSEMBLY)
    Finition (no value)
    Niveau Bas Assemblage/Elément béton = "+4.794" (IFCLABEL)
    Niveau Haut Assemblage/Elément béton = "+5.357" (IFCLABEL)
    Poids Assemblage/Elément béton = 66.3 (IFCMASSMEASURE) [KILO GRAM]
    Poids ferraillage Elément béton (no value)
    Position maillage Assemblage/Elément béton = "7-11/C-D" (IFCLABEL)
    Repère Assemblage/Elément béton = "PA27(?)" (IFCLABEL)
  Tekla Assemblages | properties | on 3 objects (3 IFCELEMENTASSEMBLY)
    Finition (no value)
    Niveau Bas Assemblage/Elément béton = "+4.794" (IFCLABEL)
    Niveau Haut Assemblage/Elément béton = "+5.357" (IFCLABEL)
    Poids Assemblage/Elément béton = 66.3 (IFCMASSMEASURE) [KILO GRAM]
    Poids ferraillage Elément béton (no value)
    Position maillage Assemblage/Elément béton = "7-11/D-E" (IFCLABEL)
    Repère Assemblage/Elément béton = "PA27(?)" (IFCLABEL)
  Tekla Assemblages | properties | on 3 objects (3 IFCELEMENTASSEMBLY)
    Finition (no value)
    Niveau Bas Assemblage/Elément béton = "+4.794" (IFCLABEL)
    Niveau Haut Assemblage/Elément béton = "+5.357" (IFCLABEL)
    Poids Assemblage/Elément béton = 66.3 (IFCMASSMEASURE) [KILO GRAM]
    Poids ferraillage Elément béton (no value)
    Position maillage Assemblage/Elément béton = "7-11/E-F" (IFCLABEL)
    Repère Assemblage/Elément béton = "PA27(?)" (IFCLABEL)
  Tekla Assemblages | properties | on 3 objects (3 IFCELEMENTASSEMBLY)
    Finition (no value)
    Niveau Bas Assemblage/Elément béton = "+4.794" (IFCLABEL)
    Niveau Haut Assemblage/Elément béton = "+5.357" (IFCLABEL)
    Poids Assemblage/Elément béton = 66.3 (IFCMASSMEASURE) [KILO GRAM]
    Poids ferraillage Elément béton (no value)
    Position maillage Assemblage/Elément béton = "7-11/F-G" (IFCLABEL)
    Repère Assemblage/Elément béton = "PA27(?)" (IFCLABEL)
  Tekla Assemblages | properties | on 3 objects (3 IFCELEMENTASSEMBLY)
    Finition (no value)
    Niveau Bas Assemblage/Elément béton = "+4.794" (IFCLABEL)
    Niveau Haut Assemblage/Elément béton = "+5.357" (IFCLABEL)
    Poids Assemblage/Elément béton = 66.3 (IFCMASSMEASURE) [KILO GRAM]
    Poids ferraillage Elément béton (no value)
    Position maillage Assemblage/Elément béton = "7-11/G-H" (IFCLABEL)
    Repère Assemblage/Elément béton = "PA27(?)" (IFCLABEL)
  Tekla Assemblages | properties | on 3 objects (3 IFCELEMENTASSEMBLY)
    Finition (no value)
    Niveau Bas Assemblage/Elément béton = "+4.794" (IFCLABEL)
    Niveau Haut Assemblage/Elément béton = "+5.357" (IFCLABEL)
    Poids Assemblage/Elément béton = 66.3 (IFCMASSMEASURE) [KILO GRAM]
    Poids ferraillage Elément béton (no value)
    Position maillage Assemblage/Elément béton = "7-11/H-I" (IFCLABEL)
    Repère Assemblage/Elément béton = "PA27(?)" (IFCLABEL)
  Tekla Assemblages: 420 more contents on 483 objects not shown
  BaseQuantities | quantities | on 126 objects (126 IFCELEMENTASSEMBLY)
    Width = 436.5 [MILLI METRE]
  BaseQuantities | quantities | on 79 objects (79 IFCBEAM)
    Length = 6000. [MILLI METRE]
    NetVolume = 0.00400948800864979 [CUBIC_METRE]
    NetWeight = 31.4744808679009 [KILO GRAM]
    OuterSurfaceArea = 8.030976036E-06 [SQUARE_METRE]
  BaseQuantities | quantities | on 50 objects (50 IFCELEMENTASSEMBLY)
    Width = 1034.70788574219 [MILLI METRE]
  BaseQuantities | quantities | on 36 objects (36 IFCBEAM)
    Length = 6500. [MILLI METRE]
    NetVolume = 0.00434361200937063 [CUBIC_METRE]
    NetWeight = 34.0973542735594 [KILO GRAM]
    OuterSurfaceArea = 8.700224039E-06 [SQUARE_METRE]
  BaseQuantities | quantities | on 24 objects (24 IFCBEAM)
    Length = 6799.99999999733 [MILLI METRE]
    NetVolume = 0.00844973531573998 [CUBIC_METRE]
    NetWeight = 66.3304222285588 [KILO GRAM]
    OuterSurfaceArea = 1.69130812711934E-05 [SQUARE_METRE]
  BaseQuantities | quantities | on 19 objects (19 IFCELEMENTASSEMBLY)
    Width = 25.4091853470345 [MILLI METRE]
  BaseQuantities | quantities | on 19 objects (19 IFCELEMENTASSEMBLY)
    Width = 25.4091853470245 [MILLI METRE]
  BaseQuantities | quantities | on 16 objects (16 IFCELEMENTASSEMBLY)
    Width = 25.4091853470272 [MILLI METRE]
  BaseQuantities: 458 more contents on 756 objects not shown
  Tekla Commun | properties | on 25 objects (25 IFCBEAM)
    Classe = "3" (IFCLABEL)
    Finition = "" (IFCLABEL)
    GUID Initial (no value)
    Matériau = "S235JR" (IFCLABEL)
    Niveau bas = "+4.794" (IFCLABEL)
    Niveau haut = "+5.357" (IFCLABEL)
    Nom = "COUVERTURE" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Profil = "BACACIER_COVEO 4.40" (IFCLABEL)
    Repère d'assemblage = "PA27(?)" (IFCLABEL)
    Repère de pièce = "PA27(?)" (IFCLABEL)
    Repère préliminaire = "" (IFCLABEL)
  Tekla Commun | properties | on 25 objects (25 IFCBEAM)
    Classe = "3" (IFCLABEL)
    Finition = "" (IFCLABEL)
    GUID Initial (no value)
    Matériau = "S235JR" (IFCLABEL)
    Niveau bas = "+4.794" (IFCLABEL)
    Niveau haut = "+5.357" (IFCLABEL)
    Nom = "COUVERTURE" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Profil = "BACACIER_COVEO 4.40" (IFCLABEL)
    Repère d'assemblage = "PA27" (IFCLABEL)
    Repère de pièce = "PA27" (IFCLABEL)
    Repère préliminaire = "" (IFCLABEL)
  Tekla Commun | properties | on 16 objects (16 IFCBEAM)
    Classe = "13" (IFCLABEL)
    Finition = "" (IFCLABEL)
    GUID Initial (no value)
    Matériau = "S235JR" (IFCLABEL)
    Niveau bas = "+5.048" (IFCLABEL)
    Niveau haut = "+5.074" (IFCLABEL)
    Nom = "ECROU_M14" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Profil = "ECROU_M14" (IFCLABEL)
    Repère d'assemblage = "PA28" (IFCLABEL)
    Repère de pièce = "PA28" (IFCLABEL)
    Repère préliminaire = "" (IFCLABEL)
  Tekla Commun | properties | on 16 objects (16 IFCBEAM)
    Classe = "13" (IFCLABEL)
    Finition = "" (IFCLABEL)
    GUID Initial (no value)
    Matériau = "S235JR" (IFCLABEL)
    Niveau bas = "+5.184" (IFCLABEL)
    Niveau haut = "+5.210" (IFCLABEL)
    Nom = "ECROU_M14" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Profil = "ECROU_M14" (IFCLABEL)
    Repère d'assemblage = "PA28" (IFCLABEL)
    Repère de pièce = "PA28" (IFCLABEL)
    Repère préliminaire = "" (IFCLABEL)
  Tekla Commun | properties | on 16 objects (16 IFCBEAM)
    Classe = "13" (IFCLABEL)
    Finition = "" (IFCLABEL)
    GUID Initial (no value)
    Matériau = "S235JR" (IFCLABEL)
    Niveau bas = "+5.185" (IFCLABEL)
    Niveau haut = "+5.211" (IFCLABEL)
    Nom = "ECROU_M14" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Profil = "ECROU_M14" (IFCLABEL)
    Repère d'assemblage = "PA28" (IFCLABEL)
    Repère de pièce = "PA28" (IFCLABEL)
    Repère préliminaire = "" (IFCLABEL)
  Tekla Commun | properties | on 14 objects (14 IFCBEAM)
    Classe = "13" (IFCLABEL)
    Finition = "" (IFCLABEL)
    GUID Initial (no value)
    Matériau = "S235JR" (IFCLABEL)
    Niveau bas = "+5.047" (IFCLABEL)
    Niveau haut = "+5.073" (IFCLABEL)
    Nom = "ECROU_M14" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Profil = "ECROU_M14" (IFCLABEL)
    Repère d'assemblage = "PA29" (IFCLABEL)
    Repère de pièce = "PA29" (IFCLABEL)
    Repère préliminaire = "" (IFCLABEL)
  Tekla Commun | properties | on 10 objects (10 IFCFOOTING)
    Classe = "8" (IFCLABEL)
    Finition = "" (IFCLABEL)
    GUID Initial (no value)
    Matériau = "C20/25" (IFCLABEL)
    Niveau bas = "-0.510" (IFCLABEL)
    Niveau haut = "-0.010" (IFCLABEL)
    Nom = "SEMELLE" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Profil = "800*800" (IFCLABEL)
    Repère d'assemblage = "S0(?)" (IFCLABEL)
    Repère de pièce = "S0(?)" (IFCLABEL)
    Repère préliminaire = "" (IFCLABEL)
  Tekla Commun | properties | on 8 objects (8 IFCBEAM)
    Classe = "13" (IFCLABEL)
    Finition = "" (IFCLABEL)
    GUID Initial (no value)
    Matériau = "S235JR" (IFCLABEL)
    Niveau bas = "+4.891" (IFCLABEL)
    Niveau haut = "+4.914" (IFCLABEL)
    Nom = "ECROU_M14" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Profil = "ECROU_M14" (IFCLABEL)
    Repère d'assemblage = "PA28" (IFCLABEL)
    Repère de pièce = "PA28" (IFCLABEL)
    Repère préliminaire = "" (IFCLABEL)
  Tekla Commun: 218 more contents on 488 objects not shown
  Tekla Quantités | properties | on 128 objects (128 IFCBEAM)
    Hauteur = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Longueur = 13. (IFCLENGTHMEASURE) [MILLI METRE]
    Poids = 0. (IFCMASSMEASURE) [KILO GRAM]
    Surface nette = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Surface par tonne = 42.8 (IFCAREAMEASURE) [SQUARE_METRE]
    Surface supérieure totale = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Tekla Quantités | properties | on 79 objects (79 IFCBEAM)
    Hauteur = 91. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur = 436.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Longueur = 6000. (IFCLENGTHMEASURE) [MILLI METRE]
    Poids = 31.5 (IFCMASSMEASURE) [KILO GRAM]
    Surface nette = 8. (IFCAREAMEASURE) [SQUARE_METRE]
    Surface par tonne = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Surface supérieure totale = 0.3 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Tekla Quantités | properties | on 50 objects (50 IFCBEAM)
    Hauteur = 41. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur = 1034.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Longueur = 6800. (IFCLENGTHMEASURE) [MILLI METRE]
    Poids = 66.3 (IFCMASSMEASURE) [KILO GRAM]
    Surface nette = 16.9 (IFCAREAMEASURE) [SQUARE_METRE]
    Surface par tonne = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Surface supérieure totale = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Tekla Quantités | properties | on 38 objects (38 IFCBEAM)
    Hauteur = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur = 8. (IFCLENGTHMEASURE) [MILLI METRE]
    Longueur = 223.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Poids = 1.6 (IFCMASSMEASURE) [KILO GRAM]
    Surface nette = 0.1 (IFCAREAMEASURE) [SQUARE_METRE]
    Surface par tonne = 35.3 (IFCAREAMEASURE) [SQUARE_METRE]
    Surface supérieure totale = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Tekla Quantités | properties | on 36 objects (36 IFCBEAM)
    Hauteur = 91. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur = 436.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Longueur = 6500. (IFCLENGTHMEASURE) [MILLI METRE]
    Poids = 34.1 (IFCMASSMEASURE) [KILO GRAM]
    Surface nette = 8.7 (IFCAREAMEASURE) [SQUARE_METRE]
    Surface par tonne = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Surface supérieure totale = 0.3 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Tekla Quantités | properties | on 20 objects (20 IFCDISCRETEACCESSORY)
    Hauteur = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Longueur = 220. (IFCLENGTHMEASURE) [MILLI METRE]
    Poids = 1. (IFCMASSMEASURE) [KILO GRAM]
    Surface nette = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Surface par tonne = 27.4 (IFCAREAMEASURE) [SQUARE_METRE]
    Surface supérieure totale = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Tekla Quantités | properties | on 16 objects (16 IFCBEAM)
    Hauteur = 60. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    Longueur = 196.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Poids = 0.5 (IFCMASSMEASURE) [KILO GRAM]
    Surface nette = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Surface par tonne = 57. (IFCAREAMEASURE) [SQUARE_METRE]
    Surface supérieure totale = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Tekla Quantités | properties | on 16 objects (16 IFCBEAM)
    Hauteur = 14. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur = 14. (IFCLENGTHMEASURE) [MILLI METRE]
    Longueur = 2205.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Poids = 2.4 (IFCMASSMEASURE) [KILO GRAM]
    Surface nette = 0.1 (IFCAREAMEASURE) [SQUARE_METRE]
    Surface par tonne = 39.5 (IFCAREAMEASURE) [SQUARE_METRE]
    Surface supérieure totale = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Tekla Quantités: 59 more contents on 235 objects not shown
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "A3(?)" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 82 objects (82 IFCBEAM)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "PA28" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 78 objects (78 IFCBEAM)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "A15" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 36 objects (36 IFCBEAM)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "A17" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 32 objects (32 IFCBEAM)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "A4" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 25 objects (25 IFCBEAM)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "PA27(?)" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 25 objects (25 IFCBEAM)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "PA27" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 22 objects (22 IFCBEAM)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "EC1" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 16 objects (16 IFCBEAM)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "LI1" (IFCIDENTIFIER)
  Pset_BeamCommon: 71 more contents on 156 objects not shown
  Tekla Ferraillage | properties | on 10 objects (10 IFCREINFORCINGBAR)
    Classe = "14" (IFCLABEL)
    Dimension = "HA16" (IFCIDENTIFIER)
    Espacements = "2x245" (IFCLABEL)
    Forme = "21" (IFCIDENTIFIER)
    Longueur = 1145. (IFCLENGTHMEASURE) [MILLI METRE]
    Nom = "FER_SUP" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Poids = 1.8 (IFCMASSMEASURE) [KILO GRAM]
    Poids total = 5.4 (IFCMASSMEASURE) [KILO GRAM]
    Qualité = "FeE500" (IFCLABEL)
    Quantité totale = 3 (IFCINTEGER)
    Repère armature = "0(?)" (IFCIDENTIFIER)
    Repère élément béton = "S0(?)" (IFCLABEL)
    TD (no value)
    a = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    b = 722. (IFCLENGTHMEASURE) [MILLI METRE]
    c = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    d (no value)
    e (no value)
    f (no value)
    g (no value)
    h1 (no value)
    h2 (no value)
    i (no value)
    j (no value)
    k1 (no value)
    k2 (no value)
    o (no value)
    r = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    s (no value)
    t (no value)
    u (no value)
    v (no value)
    x (no value)
    y (no value)
  Tekla Ferraillage | properties | on 10 objects (10 IFCREINFORCINGBAR)
    Classe = "9" (IFCLABEL)
    Dimension = "HA16" (IFCIDENTIFIER)
    Espacements = "2x294" (IFCLABEL)
    Forme = "21" (IFCIDENTIFIER)
    Longueur = 960. (IFCLENGTHMEASURE) [MILLI METRE]
    Nom = "FER_SUP" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Poids = 1.5 (IFCMASSMEASURE) [KILO GRAM]
    Poids total = 4.5 (IFCMASSMEASURE) [KILO GRAM]
    Qualité = "FeE500" (IFCLABEL)
    Quantité totale = 3 (IFCINTEGER)
    Repère armature = "0(?)" (IFCIDENTIFIER)
    Repère élément béton = "S0(?)" (IFCLABEL)
    TD (no value)
    a = 232. (IFCLENGTHMEASURE) [MILLI METRE]
    b = 572. (IFCLENGTHMEASURE) [MILLI METRE]
    c = 232. (IFCLENGTHMEASURE) [MILLI METRE]
    d (no value)
    e (no value)
    f (no value)
    g (no value)
    h1 (no value)
    h2 (no value)
    i (no value)
    j (no value)
    k1 (no value)
    k2 (no value)
    o (no value)
    r = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    s (no value)
    t (no value)
    u (no value)
    v (no value)
    x (no value)
    y (no value)
  Tekla Ferraillage | properties | on 10 objects (10 IFCREINFORCINGBAR)
    Classe = "13" (IFCLABEL)
    Dimension = "HA20" (IFCIDENTIFIER)
    Espacements = "2x292" (IFCLABEL)
    Forme = "21" (IFCIDENTIFIER)
    Longueur = 1210. (IFCLENGTHMEASURE) [MILLI METRE]
    Nom = "FER_INF" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Poids = 3. (IFCMASSMEASURE) [KILO GRAM]
    Poids total = 9. (IFCMASSMEASURE) [KILO GRAM]
    Qualité = "FeE500" (IFCLABEL)
    Quantité totale = 3 (IFCINTEGER)
    Repère armature = "0(?)" (IFCIDENTIFIER)
    Repère élément béton = "S0(?)" (IFCLABEL)
    TD (no value)
    a = 382. (IFCLENGTHMEASURE) [MILLI METRE]
    b = 572. (IFCLENGTHMEASURE) [MILLI METRE]
    c = 382. (IFCLENGTHMEASURE) [MILLI METRE]
    d (no value)
    e (no value)
    f (no value)
    g (no value)
    h1 (no value)
    h2 (no value)
    i (no value)
    j (no value)
    k1 (no value)
    k2 (no value)
    o (no value)
    r = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    s (no value)
    t (no value)
    u (no value)
    v (no value)
    x (no value)
    y (no value)
  Tekla Ferraillage | properties | on 10 objects (10 IFCREINFORCINGBAR)
    Classe = "13" (IFCLABEL)
    Dimension = "HA16" (IFCIDENTIFIER)
    Espacements = "1x194 + 1x200 + 1x194" (IFCLABEL)
    Forme = "21" (IFCIDENTIFIER)
    Longueur = 1485. (IFCLENGTHMEASURE) [MILLI METRE]
    Nom = "FER_INF" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Poids = 2.3 (IFCMASSMEASURE) [KILO GRAM]
    Poids total = 9.4 (IFCMASSMEASURE) [KILO GRAM]
    Qualité = "FeE500" (IFCLABEL)
    Quantité totale = 4 (IFCINTEGER)
    Repère armature = "0(?)" (IFCIDENTIFIER)
    Repère élément béton = "S0(?)" (IFCLABEL)
    TD (no value)
    a = 407. (IFCLENGTHMEASURE) [MILLI METRE]
    b = 750. (IFCLENGTHMEASURE) [MILLI METRE]
    c = 407. (IFCLENGTHMEASURE) [MILLI METRE]
    d (no value)
    e (no value)
    f (no value)
    g (no value)
    h1 (no value)
    h2 (no value)
    i (no value)
    j (no value)
    k1 (no value)
    k2 (no value)
    o (no value)
    r = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    s (no value)
    t (no value)
    u (no value)
    v (no value)
    x (no value)
    y (no value)
  Tekla Ferraillage | properties | on 1 object (1 IFCREINFORCINGBAR)
    Classe = "1" (IFCLABEL)
    Dimension = "HA5.5/HA5.5-200/200-13800/24800" (IFCIDENTIFIER)
    Espacements = "68x200" (IFCLABEL)
    Forme = "" (IFCIDENTIFIER)
    Longueur = 24800. (IFCLENGTHMEASURE) [MILLI METRE]
    Nom = "TREILLIS_SOUDE" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Poids = 628. (IFCMASSMEASURE) [KILO GRAM]
    Poids total = 628. (IFCMASSMEASURE) [KILO GRAM]
    Qualité = "FeE500" (IFCLABEL)
    Quantité totale = 1 (IFCINTEGER)
    Repère armature = "T/0(?)" (IFCIDENTIFIER)
    Repère élément béton = "Da0(?)" (IFCLABEL)
    TD = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    a = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    b = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    c = 5200. (IFCLENGTHMEASURE) [MILLI METRE]
    d = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    e = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    f = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    g = 5200. (IFCLENGTHMEASURE) [MILLI METRE]
    h1 (no value)
    h2 (no value)
    i (no value)
    j (no value)
    k1 (no value)
    k2 (no value)
    o (no value)
    r = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    s = 90. (IFCREAL)
    t = 90. (IFCREAL)
    u = 90. (IFCREAL)
    v = 90. (IFCREAL)
    x (no value)
    y (no value)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Da0(?)" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 16 objects (16 IFCDISCRETEACCESSORY)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "F2" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 8 objects (8 IFCPLATE)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "G14" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 8 objects (8 IFCDISCRETEACCESSORY)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "F3" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 6 objects (6 IFCDISCRETEACCESSORY)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "8" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 6 objects (6 IFCDISCRETEACCESSORY)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "F1" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 6 objects (6 IFCDISCRETEACCESSORY)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "5" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 5 objects (5 IFCDISCRETEACCESSORY)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "10" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 4 objects (4 IFCDISCRETEACCESSORY)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "71" (IFCIDENTIFIER)
  Pset_PlateCommon: 31 more contents on 64 objects not shown
  Tekla Boulons | properties | on 120 objects (120 IFCMECHANICALFASTENER)
    Diamètre = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre du trou = 13. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre rondelle = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Lieu Boulonnage = "Montage" (IFCLABEL)
    Longueur = 35. (IFCLENGTHMEASURE) [MILLI METRE]
    Nom = "M12*35" (IFCLABEL)
    Nom rondelle = "RONDELLE-M12-PLA-6.8" (IFCLABEL)
    Nom écrou = "ECROU-M12-E-6.8" (IFCLABEL)
    Quantité = 1 (IFCINTEGER)
    Quantité d'écrou = 1 (IFCINTEGER)
    Quantité de rondelle = 1 (IFCINTEGER)
    Standard = "6.8" (IFCLABEL)
    Trou oblong X = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trou oblong Y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type rondelle = "PLA-6.8" (IFCLABEL)
    Type écrou = "E-6.8" (IFCLABEL)
  Tekla Boulons | properties | on 44 objects (44 IFCMECHANICALFASTENER)
    Diamètre = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre du trou = 14. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre rondelle = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Lieu Boulonnage = "Montage" (IFCLABEL)
    Longueur = 35. (IFCLENGTHMEASURE) [MILLI METRE]
    Nom = "M12*35" (IFCLABEL)
    Nom rondelle = "RONDELLE-M12-PLA-6.8" (IFCLABEL)
    Nom écrou = "ECROU-M12-E-6.8" (IFCLABEL)
    Quantité = 1 (IFCINTEGER)
    Quantité d'écrou = 1 (IFCINTEGER)
    Quantité de rondelle = 1 (IFCINTEGER)
    Standard = "6.8" (IFCLABEL)
    Trou oblong X = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trou oblong Y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type rondelle = "PLA-6.8" (IFCLABEL)
    Type écrou = "E-6.8" (IFCLABEL)
  Tekla Boulons | properties | on 14 objects (14 IFCMECHANICALFASTENER)
    Diamètre = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre du trou = 14. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre rondelle = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Lieu Boulonnage = "Montage" (IFCLABEL)
    Longueur = 30. (IFCLENGTHMEASURE) [MILLI METRE]
    Nom = "M12*30" (IFCLABEL)
    Nom rondelle = "RONDELLE-M12-PLA-6.8" (IFCLABEL)
    Nom écrou = "ECROU-M12-E-6.8" (IFCLABEL)
    Quantité = 1 (IFCINTEGER)
    Quantité d'écrou = 1 (IFCINTEGER)
    Quantité de rondelle = 0 (IFCINTEGER)
    Standard = "6.8" (IFCLABEL)
    Trou oblong X = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trou oblong Y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type rondelle = "PLA-6.8" (IFCLABEL)
    Type écrou = "E-6.8" (IFCLABEL)
  Tekla Boulons | properties | on 10 objects (10 IFCMECHANICALFASTENER)
    Diamètre = 16. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre du trou = 18. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre rondelle = 16. (IFCLENGTHMEASURE) [MILLI METRE]
    Lieu Boulonnage = "Montage" (IFCLABEL)
    Longueur = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Nom = "M16*50" (IFCLABEL)
    Nom rondelle = "RONDELLE-M16-PLA-HR8.8" (IFCLABEL)
    Nom écrou = "ECROU-M16-E-HR8.8" (IFCLABEL)
    Quantité = 8 (IFCINTEGER)
    Quantité d'écrou = 8 (IFCINTEGER)
    Quantité de rondelle = 8 (IFCINTEGER)
    Standard = "HR8.8" (IFCLABEL)
    Trou oblong X = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trou oblong Y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type rondelle = "PLA-HR8.8" (IFCLABEL)
    Type écrou = "E-HR8.8" (IFCLABEL)
  Tekla Boulons | properties | on 4 objects (4 IFCMECHANICALFASTENER)
    Diamètre = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre du trou = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre rondelle = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Lieu Boulonnage = "Montage" (IFCLABEL)
    Longueur = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Nom = "M12*40" (IFCLABEL)
    Nom rondelle = "RONDELLE-M12-PLA-8.8" (IFCLABEL)
    Nom écrou = "ECROU-M12-E-8.8" (IFCLABEL)
    Quantité = 2 (IFCINTEGER)
    Quantité d'écrou = 2 (IFCINTEGER)
    Quantité de rondelle = 2 (IFCINTEGER)
    Standard = "8.8" (IFCLABEL)
    Trou oblong X = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trou oblong Y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type rondelle = "PLA-8.8" (IFCLABEL)
    Type écrou = "E-8.8" (IFCLABEL)
  Tekla Boulons | properties | on 3 objects (3 IFCMECHANICALFASTENER)
    Diamètre = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre du trou = 13. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre rondelle = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Lieu Boulonnage = "Montage" (IFCLABEL)
    Longueur = 35. (IFCLENGTHMEASURE) [MILLI METRE]
    Nom = "M12*35" (IFCLABEL)
    Nom rondelle = "RONDELLE-M12-PLA-8.8" (IFCLABEL)
    Nom écrou = "ECROU-M12-E-8.8" (IFCLABEL)
    Quantité = 4 (IFCINTEGER)
    Quantité d'écrou = 4 (IFCINTEGER)
    Quantité de rondelle = 4 (IFCINTEGER)
    Standard = "8.8" (IFCLABEL)
    Trou oblong X = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trou oblong Y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type rondelle = "PLA-8.8" (IFCLABEL)
    Type écrou = "E-8.8" (IFCLABEL)
  Tekla Boulons | properties | on 3 objects (3 IFCMECHANICALFASTENER)
    Diamètre = 16. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre du trou = 18. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre rondelle = 16. (IFCLENGTHMEASURE) [MILLI METRE]
    Lieu Boulonnage = "Montage" (IFCLABEL)
    Longueur = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    Nom = "M16*55" (IFCLABEL)
    Nom rondelle = "RONDELLE-M16-PLA-6.8" (IFCLABEL)
    Nom écrou = "ECROU-M16-E-6.8" (IFCLABEL)
    Quantité = 6 (IFCINTEGER)
    Quantité d'écrou = 6 (IFCINTEGER)
    Quantité de rondelle = 6 (IFCINTEGER)
    Standard = "6.8" (IFCLABEL)
    Trou oblong X = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trou oblong Y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type rondelle = "PLA-6.8" (IFCLABEL)
    Type écrou = "E-6.8" (IFCLABEL)
  Tekla Boulons | properties | on 2 objects (2 IFCMECHANICALFASTENER)
    Diamètre = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre du trou = 13. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre rondelle = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Lieu Boulonnage = "Montage" (IFCLABEL)
    Longueur = 30. (IFCLENGTHMEASURE) [MILLI METRE]
    Nom = "M12*30" (IFCLABEL)
    Nom rondelle = "RONDELLE-M12-PLA-6.8" (IFCLABEL)
    Nom écrou = "ECROU-M12-E-6.8" (IFCLABEL)
    Quantité = 1 (IFCINTEGER)
    Quantité d'écrou = 1 (IFCINTEGER)
    Quantité de rondelle = 0 (IFCINTEGER)
    Standard = "6.8" (IFCLABEL)
    Trou oblong X = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trou oblong Y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type rondelle = "PLA-6.8" (IFCLABEL)
    Type écrou = "E-6.8" (IFCLABEL)
  Tekla Boulons: 6 more contents on 10 objects not shown
  Pset_ColumnCommon | properties | on 4 objects (4 IFCCOLUMN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "1" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "64" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "67" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "40" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "44" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "44(?)" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "1(?)" (IFCIDENTIFIER)