IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2017-12-13T14:23:35"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20170927_1515(x64) - Exporter 18.2.0.0 - Interface alternative d'export 18.2.0.0"
Application: "Autodesk Revit 2018 (FRA)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (FRA)"

People and organizations
  Person "ced.dziuba@gmail.com" of Organization (no name given)
  Owner history of Person "ced.dziuba@gmail.com" of Organization (no name given) | application "Autodesk Revit 2018 (FRA)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (FRA)" | change NOCHANGE | created 1512976730 (2017-12-11T07:18:50Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT | long name "CONSTRUCTION D'UNE ECOLE A AUBAREDE (65)"
  IFCSITE "Surface:297878" | latitude 48° 52′ 53.759999″ | longitude 2° 25′ 58.079999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Entrer l'adresse ici", "Paris", "France"
      IFCBUILDINGSTOREY "1 - RDC" | long name "1 - RDC" | elevation 1.94210219716249E-13
        contains 3 elements
          1 x IFCSLAB | object type "Terre-plein:Pelouse - 360 mm" | FLOOR | names: "Terre-plein:Pelouse - 360 mm:297981" | material: layers "Terre-plein:Pelouse - 360 mm" ("Site - Herbe" 0.36) | property sets: Pset_SlabCommon
          1 x IFCSLAB | object type "Terre-plein:Grave 0,315 31 cm + Enrobé 5 cm" | FLOOR | names: "Terre-plein:Grave 0,315 31 cm + Enrobé 5 cm:298302" | material: layers "Terre-plein:Grave 0,315 31 cm + Enrobé 5 cm" ("Site - Asphalte" 0.05, "Maçonnerie - Hérisson" 0.31) | property sets: Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | object type "Portail coulissant - 02" | names: "Portail coulissant - 02:Portail coulissant - 02:317456" | material: materials ("Finition Peinture - Blanc satiné", "Peinture - Noir") | property sets: Pset_BuildingElementProxyCommon

Property sets
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Pelouse - 360 mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Grave 0,315 31 cm + Enrobé 5 cm" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Portail coulissant - 02" (IFCIDENTIFIER)